* **Check Propane Bottle Levels, fill if needed.**

Before Departure

* **Check Generator Fuel Levels, add fuel is needed (Keep in mind Fuel weight).**
* **Check RV Battery Charge.**
* **Check tow vehicle tire pressure.**
* **Check RV tire pressure.**
* **Arrange breakable items to prevent breakage and damage to the interior.**
* **Lower roof-mounted TV antenna**
* **Lower roof-mounted satellite dish (TV and Internet)**
* **Latch Shower, Pocket and Closet Doors**
* **Close all interior cabinet/pantry doors.**
* **Secure TV(s)**
* **Secure other entertainment electronics and computer accessories**
* **Close roof vents and windows (except those for ventilation)**
* **Stow and Secure Awnings**
* **Check Slide Toppers for debris and water (if applicable)**
* **Move items out of the way of slides inside RV.**
* **Move in slides a little bit (where the slide has “kicked up”) and stop. Vacuum out the open area under the slide, this will prevent debris from scratching/digging into floors.**
* **Place your black slide “slickers” down in front of the slides.**
* **Note: If you have an L-Sectional you will need to move and properly lay it down (upside down on the couch is most common) the end not sitting in the slide before pulling in the Slides.**
* **Move the Slides in completely.**
* **Lay down and pad any large items that may move or shift during travel. (example: Bar Stools, Chairs, end of L-Sectional)**
* **Turn off all A/C units.**
* **Empty black tank and close black tank valves.**
* **Empty grey tank and close grey tank valves.**
* **Add treatment Chemical as well as 1-2 Gallons of water to black tank.**
* **Disconnect sewer and water hoses and store hoses and related accessories.**
* **Turn off all RV lights to prevent unnecessary battery drainage.**
* **Confirm that the refrigerator is running off the 12-volt DC (Dedicated converter) if using an inverter. Or is turned off.**
* **Turn off all propane appliances – Water, Heater, Furnace.**
* **Follow the Hitching Guide, and Properly hitch the Tow Vehicle to the RV.**
* **Perform Safety Test “Pull” before completely raising your leveling system.**
* **Connect breakaway switch cable to tow vehicle.**
* **Attach sway bar and safety chains.**
* **Raise leveling system.**
* **Collect and store leveling blocks.**
* **Confirm that everything is “all clear” under the RV.**
* **Remove any wheel chocks.**
* **Close and Lock all external doors.**
* **Check RV and tow vehicle signal lights.**
* **Check RV brakes, (3 Methods; Press tow vehicle brake pedal; Engage RV brakes only by using trailer brake controller inside tow vehicle; pull break away switch cable on RV)**
* **Perform a final walk around; looking under and around RV.**

**Congratulations! You are ready to head out on your next Journey, be safe and have a great time!**